# V150 - Station Cell Only Observation

Base: v149_swap_row_col_from_v148.

Changes:
- Station observed height now samples only the assigned station sample cell.
- JESIM observation height now samples only mapped_grid_index.
- Removed the local-neighborhood max search for observation values.
- Kept station/JESIM 1 m shoreline-equivalent conversion for that exact cell.
- Map/max-wave output shoaling remains disabled to avoid double shoaling.
- V149 row/col swap, M0 x2, 6h 22.5% decay, face-depth flux, CSV dip-all, and station id 49 fixes are retained.

Purpose:
- Prevent observation values from borrowing a higher wave from a neighboring bay/coast cell.
- Make the displayed/CSV/JESIM observation value correspond exactly to the mapped observation cell.
